{
"ARaz1_enginemounts": {
    "information":{
        "authors":"BeamNG",
        "name":"Stock Engine Mounts",
        "value":50,
    },
    "slotType" : "ARaz1_enginemounts",
    "nodes": [
        ["id", "posX", "posY", "posZ"],
        //--1.5L I4 Engine--
        {"selfCollision":false},
        {"collision":true},
        {"nodeMaterial":"|NM_METAL"},
        {"frictionCoef":0.5},
        {"group":""},
        //engine mount slidenode
         {"group":""},
         {"nodeWeight":2.0},
         ["fx2", 0.00, -1.1919, 0.2166],
    ],
    "slidenodes": [
        ["id:", "railName", "attached", "fixToRail", "tolerance", "spring", "strength", "capStrength"],
        ["fx2", "enginemountnode", true, true, 0.0, 11001000, "FLT_MAX", "FLT_MAX"],
    ],
    "beams": [
          ["id1:", "id2:"],

          //engine soft mount
          {"optional":true},
          {"deformLimitExpansion":""},
          {"beamPrecompression":1, "beamType":"|BOUNDED", "beamLongBound":0.1, "beamShortBound":0.1,"boundZone":0.02},
          {"beamSpring":261000,"beamDamp":1000},
          {"beamLimitSpring":2001000,"beamLimitDamp":500},
          {"beamDeform":20000,"beamStrength":40000},
          {"breakGroup":"enginemount_a"},
          {"dampCutoffHz":500},
          {"boundZone":0.02},
          ["em1r", "f12rr"],
          ["em1r", "f10rr"],
          ["em1r", "f12ll", {"boundZone":0.005}],
          ["em1r", "f10ll", {"boundZone":0.005}],
          ["em1r", "f1r"],
          ["em1r", "f5r"],

          //transmission soft mount
          {"breakGroup":"enginemount_b"},
          ["em1l", "f12ll"],
          ["em1l", "f10ll"],
          ["em1l", "f12rr", {"boundZone":0.005}],
          ["em1l", "f10rr", {"boundZone":0.005}],
          ["em1l", "f1l"],
          ["em1l", "f5l"],

          //engine torque mount
          {"beamSpring":2921000,"beamDamp":3500},
          {"beamLimitSpring":2001000,"beamLimitDamp":500},
          {"beamDeform":20000,"beamStrength":20000},
          {"breakGroup":"enginemount_c"},
          {"boundZone":0.02},
          ["em2", "fx2"],
          ["em2", "fx6r"],
          ["em2", "fx6l"],
          {"boundZone":""},
          {"breakGroup":""},

          //damper
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamDeform":15000,"beamStrength":30000},
          {"beamSpring":100,"beamDamp":1000},
          {"breakGroup":"enginemount_d"},
          ["e3l", "f11rr"],
          ["e4l", "f11ll"],
          ["e4r", "f10rr"],
          ["e3r", "f10ll"],
          {"dampCutoffHz":""},
          //damper break
          {"beamSpring":0,"beamDamp":0},
          {"beamPrecompression":1, "beamType":"|SUPPORT", "beamLongBound":2.0},
          ["e3l", "f11rr"],
          ["e4l", "f11ll"],
          ["e4r", "f10rr"],
          ["e3r", "f10ll"],
          {"breakGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0,"boundZone":""},
    ],
},
"ARaz1_enginemounts_heavy": {
    "information":{
        "authors":"BeamNG",
        "name":"Heavy Duty Engine Mounts",
        "value":220,
    },
    "slotType" : "ARaz1_enginemounts",
    "nodes": [
        ["id", "posX", "posY", "posZ"],
        //--1.5L I4 Engine--
        {"selfCollision":false},
        {"collision":true},
        {"nodeMaterial":"|NM_METAL"},
        {"frictionCoef":0.5},
        {"group":""},
        //engine mount slidenode
         {"group":""},
         {"nodeWeight":2.0},
         ["fx2", 0.00, -1.1919, 0.2166],
    ],
    "slidenodes": [
        ["id:", "railName", "attached", "fixToRail", "tolerance", "spring", "strength", "capStrength"],
        ["fx2", "enginemountnode", true, true, 0.0, 11001000, "FLT_MAX", "FLT_MAX"],
    ],
    "beams": [
          ["id1:", "id2:"],

          //engine soft mount
          {"optional":true},
          {"deformLimitExpansion":""},
          {"beamPrecompression":1, "beamType":"|BOUNDED", "beamLongBound":0, "beamShortBound":0},
          {"beamSpring":1531000,"beamDamp":1000},
          {"beamLimitSpring":4001000,"beamLimitDamp":500},
          {"beamDeform":40000,"beamStrength":90000},
          {"breakGroup":"enginemount_a"},
          {"dampCutoffHz":500},
          {"boundZone":0.01},
          ["em1r", "f12rr"],
          ["em1r", "f10rr"],
          ["em1r", "f12ll", {"boundZone":0.005}],
          ["em1r", "f10ll", {"boundZone":0.005}],
          ["em1r", "f1r"],
          ["em1r", "f5r"],

          //transmission soft mount
          {"breakGroup":"enginemount_b"},
          ["em1l", "f12ll"],
          ["em1l", "f10ll"],
          ["em1l", "f12rr", {"boundZone":0.005}],
          ["em1l", "f10rr", {"boundZone":0.005}],
          ["em1l", "f1l"],
          ["em1l", "f5l"],

          //solid engine torque mount
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
          {"beamSpring":2921000,"beamDamp":400},
          {"beamDeform":70000,"beamStrength":120000},
          {"breakGroup":"enginemount_c"},
          ["em2", "fx2r"],
          ["em2", "fx2l"],
          ["em2", "fx2"],
          ["em2", "fx6r"],
          ["em2", "fx6l"],
          {"boundZone":""},
          {"breakGroup":""},

          //damper
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
          {"beamDeform":15000,"beamStrength":60000},
          {"beamSpring":100,"beamDamp":3000},
          {"breakGroup":"enginemount_d"},
          ["e3l", "f11rr"],
          ["e4l", "f11ll"],
          ["e4r", "f10rr"],
          ["e3r", "f10ll"],
          {"dampCutoffHz":""},
          //damper break
          {"beamSpring":0,"beamDamp":0},
          {"beamPrecompression":1, "beamType":"|SUPPORT", "beamLongBound":2.0},
          ["e3l", "f11rr"],
          ["e4l", "f11ll"],
          ["e4r", "f10rr"],
          ["e3r", "f10ll"],
          {"breakGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"ARaz1_enginemounts_ultra": {
    "information":{
        "authors":"BeamNG",
        "name":"Ultra Heavy Duty Engine Mounts",
        "value":500,
    },
    "slotType" : "ARaz1_enginemounts",
    "nodes": [
        ["id", "posX", "posY", "posZ"],
        //--1.5L I4 Engine--
        {"selfCollision":false},
        {"collision":true},
        {"nodeMaterial":"|NM_METAL"},
        {"frictionCoef":0.5},
        {"group":""},
        //engine mount nodes
        ["em2",0.0, -1.12, 0.5, {"nodeWeight":8}],
        //engine mount slidenode
         {"group":""},
         {"nodeWeight":2.0},
         ["fx2", 0.00, -1.1919, 0.2166],
    ],
    "slidenodes": [
        ["id:", "railName", "attached", "fixToRail", "tolerance", "spring", "strength", "capStrength"],
        ["fx2", "enginemountnode", true, true, 0.0, 11001000, "FLT_MAX", "FLT_MAX"],
    ],
    "beams": [
          ["id1:", "id2:"],

          //engine solid  mount
          {"optional":true},
          {"deformLimitExpansion":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":3501000,"beamDamp":900},
          {"beamDeform":60000,"beamStrength":120000},
          {"breakGroup":"enginemount_a"},
          {"dampCutoffHz":500},
          ["em1r", "f12rr"],
          ["em1r", "f10rr"],
          ["em1r", "f12ll"],
          ["em1r", "f10ll"],
          ["em1r", "f1r"],
          ["em1r", "f5r"],

          //transmission soft mount
          {"breakGroup":"enginemount_b"},
          ["em1l", "f12ll"],
          ["em1l", "f10ll"],
          ["em1l", "f12rr"],
          ["em1l", "f10rr"],
          ["em1l", "f1l"],
          ["em1l", "f5l"],

          //engine torque mount
          {"beamSpring":8001000,"beamDamp":400},
          {"beamDeform":110000,"beamStrength":180000},
          {"breakGroup":"enginemount_c"},
          ["em2", "fx2"],
          ["em2", "fx6r"],
          ["em2", "fx6l"],
          {"boundZone":""},
          {"breakGroup":""},

          //damper
          {"beamDeform":15000,"beamStrength":60000},
          {"beamSpring":100,"beamDamp":500},
          {"breakGroup":"enginemount_d"},
          ["e3l", "f11rr"],
          ["e4l", "f11ll"],
          ["e4r", "f10rr"],
          ["e3r", "f10ll"],
          ["e4r", "f10rr"],
          ["e4r", "f11rr"],
          ["airb2", "f11ll"],
          ["e3r", "f10ll"],
          ["e3l", "f10ll"],
          ["e3l", "f1l"],
          ["e4l", "f10rr"],
          ["e4l", "f1r"],
          {"dampCutoffHz":""},
          //damper break
          {"beamSpring":0,"beamDamp":0},
          {"beamPrecompression":1, "beamType":"|SUPPORT", "beamLongBound":2.0},
          ["e3l", "f11rr"],
          ["e4l", "f11ll"],
          ["e4r", "f10rr"],
          ["e3r", "f10ll"],
          {"breakGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"ARaz1_enginemounts_midengine": {
    "information":{
        "authors":"BeamNG",
        "name":"Stock Engine Mounts",
        "value":650,
    },
    "slotType" : "ARaz1_enginemounts_midengine",
    "beams": [
          ["id1:", "id2:"],

          //engine soft mount
          {"optional":true},
          {"deformLimitExpansion":""},
          {"beamPrecompression":1, "beamType":"|BOUNDED", "beamLongBound":0.3, "beamShortBound":0.3,"boundZone":0.1},
          {"beamSpring":4001000, "beamDamp":300},
          {"beamSpring":1225000, "beamDamp":1000},
          {"beamDeform":75000, "beamStrength":50000},
          {"dampCutoffHz":500},
          {"boundZone":0.01},
          {"breakGroup":"enginemount_R"},
          ["em1r", "rx1r"],
          ["em1r", "f3r"],
          ["em1r", "f8r"],
          ["em1r", "rx3r"],
          ["em1r", "rx1l"],
          ["em1r", "f3l"],
          ["e1r", "f3r"],
          ["e2r", "rx1r"],
          {"breakGroup":"enginemount_L"},
          ["em1l", "rx1l"],
          ["em1l", "f3l"],
          ["em1l", "f8l"],
          ["em1l", "rx3l"],
          ["em1l", "rx1r"],
          ["em1l", "f3r"],
          ["e1l", "f3l"],
          ["e2l", "rx1l"],

          //transmission mount
          {"boundZone":0.01},
          {"breakGroup":"transmissionmount_R"},
          ["tm1r", "rx2r"],
          ["tm1r", "rx4r"],
          ["tm1r", "rx1r"],
          ["tm1r", "rx3r"],
          ["tm1r", "rx2"],
          ["tm1r", "rx1"],
          {"breakGroup":"transmissionmount_L"},
          ["tm1l", "rx2l"],
          ["tm1l", "rx4l"],
          ["tm1l", "rx1l"],
          ["tm1l", "rx3l"],
          ["tm1l", "rx2"],
          ["tm1l", "rx1"],
          {"boundZone":""},
          {"breakGroup":""},

          //damper
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamDeform":15000, "beamStrength":42000},
          {"beamSpring":45000, "beamDamp":2500},
          ["e4l", "rx3r"],
          ["e3l", "f8r"],
          ["e3r", "f8l"],
          ["e4r", "rx3l"],
          ["e3r", "f3r"],
          ["e3l", "f3l"],
          ["e1r", "f8r"],
          ["e1l", "f8l"],
          ["e2r", "rx3r"],
          ["e2l", "rx3l"],
          ["e4l", "rx1l"],
          ["e4r", "rx1r"],

          ["tra3", "rx3l"],
          ["tra3", "rx3r"],
          ["tra3", "rx2l"],
          ["tra3", "rx2r"],
          {"dampCutoffHz":""},
          {"optional":false},

          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0,"boundZone":""},
    ],
},
"ARaz1_enginemounts_ultra_midengine": {
    "information":{
        "authors":"BeamNG",
        "name":"Ultra Heavy Duty Engine Mounts",
        "value":2500,
    },
    "slotType" : "ARaz1_enginemounts_midengine",
    "beams": [
          ["id1:", "id2:"],

          //engine solid mounts
          {"optional":true},
          {"deformLimitExpansion":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":5001000, "beamDamp":300},
          {"beamDeform":125000, "beamStrength":160000},
          {"dampCutoffHz":500},
          {"breakGroup":"enginemount_R"},
          ["em1r", "rx1r"],
          ["em1r", "f3r"],
          ["em1r", "f8r"],
          ["em1r", "rx3r"],
          ["em1r", "rx1l"],
          ["em1r", "f3l"],
          ["e1r", "f3r"],
          ["e2r", "rx1r"],
          {"breakGroup":"enginemount_L"},
          ["em1l", "rx1l"],
          ["em1l", "f3l"],
          ["em1l", "f8l"],
          ["em1l", "rx3l"],
          ["em1l", "rx1r"],
          ["em1l", "f3r"],
          ["e1l", "f3l"],
          ["e2l", "rx1l"],

          //transmission mount
          {"beamSpring":4001000, "beamDamp":400},
          {"breakGroup":"transmissionmount_R"},
          ["tm1r", "rx2r"],
          ["tm1r", "rx4r"],
          ["tm1r", "rx1r"],
          ["tm1r", "rx3r"],
          ["tm1r", "rx2"],
          ["tm1r", "rx1"],
          {"breakGroup":"transmissionmount_L"},
          ["tm1l", "rx2l"],
          ["tm1l", "rx4l"],
          ["tm1l", "rx1l"],
          ["tm1l", "rx3l"],
          ["tm1l", "rx2"],
          ["tm1l", "rx1"],
          {"boundZone":""},
          {"breakGroup":""},

          //damper
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamDeform":15000, "beamStrength":42000},
          {"beamSpring":45000, "beamDamp":1000},
          ["e4l", "rx3r"],
          ["e3l", "f8r"],
          ["e3r", "f8l"],
          ["e4r", "rx3l"],
          ["e3r", "f3r"],
          ["e3l", "f3l"],
          ["e1r", "f8r"],
          ["e1l", "f8l"],
          ["e2r", "rx3r"],
          ["e2l", "rx3l"],
          ["e4l", "rx1l"],
          ["e4r", "rx1r"],

          ["tra3", "rx3l"],
          ["tra3", "rx3r"],
          ["tra3", "rx2l"],
          ["tra3", "rx2r"],
          {"dampCutoffHz":""},
          {"optional":false},

          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
}