{
"ARaz1_suspension_F": {
    "information":{
        "authors":"BeamNG",
        "name":"Independent Front Suspension",
        "value":450,
    },
    "slotType" : "ARaz1_suspension_F",
    "slots": [
        ["type", "default", "description"],
        ["ARaz1_hub_F","ARaz1_hub_F_4", "Front Wheel Hubs"],
        ["ARaz1_wheeldata_F","ARaz1_wheeldata_F", "Front Spindles"],
        ["ARaz1_coilover_F","ARaz1_coilover_F", "Front Struts"],
        ["ARaz1_swaybar_F","ARaz1_swaybar_F", "Front Sway Bar"],
        ["ARaz1_steering","ARaz1_steering", "Steering"],
    ],
    "variables": [
        ["name", "type", "unit", "category", "default", "min", "max", "title", "description"],
        ["$camber_FR", "range", "", "Wheel Alignment", 0.96, 0.53, 1.34, "Camber Adjust", "Adjusts the wheel camber angle", {"subCategory":"Front"}],
        ["$caster_FR", "range", "", "Wheel Alignment", 1, 1.02, 0.98, "Caster Adjust", "Adjusts forward rake of the steering axis", {"subCategory":"Front"}],
        ["$trackoffset_F", "range", "+m", "Wheels", 0.0, -0.02, 0.09, "Wheel Offset", "Spacing of the wheel from the hub", {"stepDis":0.001, "subCategory":"Front"}],
    ],
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        //front running gear
        ["ARaz1_subframe_F", ["ARaz1_subframe_F"]],
        ["ARaz1_subframe_F_body", ["ARaz1_framerails_F", "ARaz1_traction_rods_F_mount"]],
        ["ARaz1_upperarm_F", ["ARaz1_uppermounts_a_F","ARaz1_uppermounts_b_F","ARaz1_upperarm_F"]],
        ["ARaz1_lowerarm_F_a", ["ARaz1_lowermounts_F","ARaz1_lowerarm_F"]],
        ["ARaz1_lowerarm_F_b", ["ARaz1_lowermounts_F","ARaz1_lowerarm_F"]],
        ["ARaz1_hub_FR", ["ARaz1_hub_FR"]],
        ["ARaz1_hub_FL", ["ARaz1_hub_FL"]],
    ],
    "rails": {
        "lowerarm_FL":{"links:":["fx2l", "fh1l"], "broken:":[], "looped":false, "capped":true},
        "lowerarm_FR":{"links:":["fx2r", "fh1r"], "broken:":[], "looped":false, "capped":true},
        "enginemountnode":{"links:":["fx2r", "fx2l"], "broken:":[], "looped":false, "capped":true},
    },
    "slidenodes": [
        ["id:", "railName", "attached", "fixToRail", "tolerance", "spring", "strength", "capStrength"],
        ["fh4l", "lowerarm_FL", true, true, 0.0, 11001000, "FLT_MAX", "FLT_MAX"],
        ["fh4r", "lowerarm_FR", true, true, 0.0, 11001000, "FLT_MAX", "FLT_MAX"],

        ["arbf3l", "lowerarm_FL", true, true, 0.0, 11001000, "FLT_MAX", "FLT_MAX"],
        ["arbf3r", "lowerarm_FR", true, true, 0.0, 11001000, "FLT_MAX", "FLT_MAX"],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //--FRONT SUBFRAME--
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"collision":true},
         {"selfCollision":true},
         //double wishbone suspension
         //front suspension axis points
         //lower
         {"nodeWeight":3.5},
         {"group":["ARaz1_lowermounts_F","ARaz1_traction_rods_F_mount"]},
         ["fx1r", -0.35208, -1.62447, 0.19351],
         ["fx1l", 0.35208, -1.62447, 0.19351],
         {"group":"ARaz1_subframe_F"},
         {"nodeWeight":6.5}
         ["fx2r", -0.26104, -1.19254, 0.19946, {"group":["ARaz1_subframe_F","ARaz1_lowermounts_F"], "tag":"rideheight_FR"}],
         ["fx2l", 0.26104, -1.19254, 0.19946, {"group":["ARaz1_subframe_F","ARaz1_lowermounts_F"], "tag":"rideheight_FL"}],

         //upper control arm mounts
         {"group":["ARaz1_uppermounts_a_F","ARaz1_body"]},
         {"nodeWeight":3.5},
         //["fx3r", -0.4383, -1.3070, 0.6136],
         //["fx3l",  0.4383, -1.3070, 0.6136],
         {"group":["ARaz1_uppermounts_b_F","ARaz1_body"]},
         //["fx4r", -0.4793, -1.1286, 0.6145],
         //["fx4l",  0.4793, -1.1286, 0.6145],

         {"nodeWeight":3.0},
         {"selfCollision":false},
         {"group":"ARaz1_subframe_F"},
         ["fx6r", -0.30648, -1.20955, 0.26833,],
         ["fx6l", 0.30648, -1.20955, 0.26833],
         //steering rack
         {"nodeWeight":5.5},
         {"group":["ARaz1_subframe_F","ARaz1_steeringbox_F"]},
         ["fx5r", -0.22220, -1.10471, 0.26082],
         ["fx5l", 0.22220, -1.10471, 0.26082],


         //--FRONT INDEPENDENT SUSPENSION--
         {"collision":true},
         {"selfCollision":true},
         //front hub
         //this is the steering axis
         {"nodeWeight":5.5},
         ["fh1r", -0.54029, -1.24646, 0.19574, {"group":["ARaz1_hub_FR","ARaz1_lowerarm_F"]}],
         ["fh1l", 0.54029, -1.24646, 0.19574, {"group":["ARaz1_hub_FL","ARaz1_lowerarm_F"]}],
         {"selfCollision":false},
         {"nodeWeight":4.25},
         //["fh2r", -0.50860, -1.22150, 0.65800, {"group":["ARaz1_hub_FR","ARaz1_upperarm_F"]}],
         //["fh2l", 0.50860, -1.22150, 0.65800, {"group":["ARaz1_hub_FL","ARaz1_upperarm_F"]}],
         ["fh2r", -0.641, -1.2215, 0.658, {"group":["ARaz1_hub_FR","ARaz1_upperarm_F"]}],
         ["fh2l",  0.641, -1.2215, 0.658, {"group":["ARaz1_hub_FL","ARaz1_upperarm_F"]}],
         //tie rod goes here
         {"nodeWeight":3.75},
         //["fh3r", -0.53637, -1.12120, 0.30400, {"group":["ARaz1_hub_FR","ARaz1_tierod_F"]}],
         //["fh3l", 0.53637, -1.12120, 0.30400, {"group":["ARaz1_hub_FL","ARaz1_tierod_F"]}],
         {"selfCollision":true},
         ["fh3r", -0.6760, -1.1212, 0.304, {"group":["ARaz1_hub_FR","ARaz1_tierod_F"]}],
         ["fh3l",  0.6760, -1.1212, 0.304, {"group":["ARaz1_hub_FL","ARaz1_tierod_F"]}],
         {"nodeWeight":2.0},
         {"group":["ARaz1_shockbottom_F","ARaz1_lowerarm_F"]},
         //bottom of shock
         ["fh4r", -0.46317, -1.23157, 0.19676],
         ["fh4l", 0.46317, -1.23157, 0.19676],
         {"collision":true},
         //brake hub node
         {"group":""},
         {"nodeWeight":2.75},
         ["fh6r", -0.57082, -1.37647, 0.25760, {"group":"ARaz1_hub_FR"}],
         ["fh6l", 0.57082, -1.37647, 0.25760, {"group":"ARaz1_hub_FL"}],
         {"nodeWeight":6.5},
         //sway bar control arm nodes
         {"group":["ARaz1_swaybar_F","ARaz1_lowerarm_F"]},
         ["arbf3r", -0.40302, -1.21998, 0.19755],
         ["arbf3l", 0.40302, -1.21998, 0.19755],
         {"group":""},
    ],
    "torsionbars": [
        ["id1:", "id2:", "id3:", "id4:"],
        {"spring":110000, "damp":0, "deform":25000, "strength":100000},
        //rigidify lower control arm
        //["fh7l", "fh5l", "fx2l", "f1l"],
        //["fh7r", "fh5r", "fx2r", "f1r"],
        //prevent the lower control arm from wobling (that much) after subframe breaks off
        {"spring":1000, "damp":0, "deform":25000, "strength":100000},
        //["fh7l", "fh5l", "fx2l", "fx6l"],
        //["fh7r", "fh5r", "fx2r", "fx6r"],
        //rigidify traction bar attach
        {"spring":200000, "damp":5, "deform":70000, "strength":100000},
        ["fx1l", "f11rr", "f13rr", "f13ll"],
        ["fx1r", "f11ll", "f13ll", "f13rr"],
        {"spring":150000, "damp":0, "deform":25000, "strength":100000},
        //rigidify steering arm
        ["fw1rr", "fw1r", "fh2r", "fh3r"],
        ["fw1ll", "fw1l", "fh2l", "fh3l"],
    ],
    "beams": [
          ["id1:", "id2:"],
          //--FRONT SUBFRAME--
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
          {"beamSpring":5001000,"beamDamp":120},
          {"beamDeform":25000,"beamStrength":"FLT_MAX"},
          //main shape
          {"deformLimitExpansion":1.1},
          ["fx6r", "fx2r"],
          ["fx6l", "fx2l"],
          //["fx1r", "fx1l"],
          ["fx6r", "fx6l"],
          //crossing
          {"deformLimitExpansion":""},
          {"beamDeform":16000,"beamStrength":"FLT_MAX"},
          ["fx2r", "fx6l"],
          ["fx2l", "fx6r"],

          //steering box
          {"beamDeform":45000,"beamStrength":"FLT_MAX"},
          {"deformLimitExpansion":1.1},
          ["fx5r","fx5l"],
          {"beamDeform":25000,"beamStrength":"FLT_MAX"},
          ["fx5r","fx6r"],
          ["fx5l","fx6l"],
          ["fx5r","fx2r"],
          ["fx5l","fx2l"],
          {"deformLimitExpansion":""},
          ["fx5r","fx2l"],
          ["fx5l","fx2r"],
          ["fx5l", "fx6r"],
          ["fx5r", "fx6l"],

          //engine mount node
          {"beamSpring":1001000,"beamDamp":50},
          {"beamDeform":9000,"beamStrength":"FLT_MAX"},
          {"optional":true},
          ["fx2", "fx2r"],
          ["fx2", "fx2l"],
          ["fx2", "fx6r"],
          ["fx2", "fx6l"],
          {"optional":false},
          //attach to body
          //rear
          {"beamSpring":4201000,"beamDamp":100},
          {"beamDeform":4500,"beamStrength":90000},
         // {"breakGroup":"subframemount_FRR"},
          ["fx2r", "f1r"],
          ["fx2r", "f5r",{"beamDeform":5500,"beamStrength":250000}],
          ["fx2r", "f1l",{"beamDeform":5500}],
          ["fx5r", "f1r"],
          ["fx5r", "f5r",{"beamDeform":5500}],
          ["fx5r", "f1l",{"beamDeform":4500}],
          {"beamDeform":2500},
          ["fx6r", "f1r"],
          ["fx6r", "f5r",{"beamDeform":5500,"beamStrength":250000}],
          {"beamDeform":19500},
          ["fx2r", "f10rr"],
          ["fx5r", "f10rr"],
          ["fx6r", "f10rr"],
          ["fx2r", "f12rr"]
          ["fx5r", "f12ll",{"beamDeform":7500}],
          ["fx5r", "f12rr"],
          ["fx6r", "f12rr"],
          {"beamSpring":4201000,"beamDamp":100},
          {"beamDeform":4500,"beamStrength":90000},
         // {"breakGroup":"subframemount_FRL"},
          ["fx2l", "f1l"],
          ["fx2l", "f5l",{"beamDeform":5500,"beamStrength":250000}],
          ["fx2l", "f1r",{"beamDeform":5500}],
          ["fx5l", "f1l"],
          ["fx5l", "f5l",{"beamDeform":5500}],
          ["fx5l", "f1r",{"beamDeform":4500}],
          {"beamDeform":2500},
          ["fx6l", "f1l"],
          ["fx6l", "f5l",{"beamDeform":5500,"beamStrength":250000}],
          {"beamDeform":19500},
          ["fx2l", "f10ll"],
          ["fx5l", "f10ll"],
          ["fx6l", "f10ll"],
          ["fx2l", "f12ll"]
          ["fx5l", "f12rr",{"beamDeform":7500}],
          ["fx5l", "f12ll"],
          ["fx6l", "f12ll"],

          //front
          {"beamSpring":4201000,"beamDamp":150},
          {"beamDeform":38000,"beamStrength":"FLT_MAX"},
          {"breakGroup":""},
          ["fx1r", "f13rr"],
          ["fx1l", "f13ll"],
          ["fx1r", "f11rr"],
          ["fx1l", "f11ll"],
          {"beamDeform":6000,"beamStrength":"FLT_MAX"},
          ["fx1r", "f11ll"],
          ["fx1l", "f11rr"],
          ["fx1l", "f11"],
          ["fx1r", "f11"],
          ["fx1r", "f19rr"],
          ["fx1l", "f19ll"],
          {"beamSpring":801000,"beamDamp":50},
          {"beamDeform":6000,"beamStrength":"FLT_MAX"},
          ["fx1l", "f12ll"],
          ["fx1l", "f10ll"],
          ["fx1r", "f12rr"],
          ["fx1r", "f10rr"],
          {"breakGroup":""},

          //limiter
          {"beamPrecompression":1.0, "beamType":"|SUPPORT", "beamLongBound":2},
          {"beamSpring":4001000,"beamDamp":180},
          {"beamDeform":2000,"beamStrength":80000},
          {"deformLimitExpansion":""},
          ["fx2r", "f6r"],
          ["fx2l", "f6l"],
          //--FRONT RUNNING GEAR--
          {"deformLimitExpansion":1.1},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          //double wishbone suspension
          {"beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamDeform":79000,"beamStrength":230000},
          {"beamSpring":7501000,"beamDamp":80},
          //front hub
          ["fh1r","fh2r"],
          ["fh1l","fh2l"],
          ["fh1r","fh3r"],
          ["fh1l","fh3l"],
          ["fh2r","fh3r"],
          ["fh2l","fh3l"],

          {"beamSpring":5501000,"beamDamp":80},
          ["fh1r","fh6r"],
          ["fh1l","fh6l"],
          ["fh2r","fh6r"],
          ["fh2l","fh6l"],
          ["fh3r","fh6r"],
          ["fh3l","fh6l"],

          //attach to wheel
          {"beamSpring":7501000,"beamDamp":80},
          {"beamDeform":108000,"beamStrength":257500},
          {"optional":true},
          {"breakGroup":"wheel_FR"},
          ["fh1r","fw1r", {"name":"axle_FR"}],
          ["fh2r","fw1r"],
          ["fh3r","fw1r", {"beamSpring":10501000,"beamDamp":15}],
          ["fh6r","fw1r", {"beamSpring":5501000,"beamDamp":15}],
          ["fh1r","fw1rr"],
          ["fh2r","fw1rr"],
          ["fh3r","fw1rr", {"beamSpring":10501000,"beamDamp":15}],
          ["fh6r","fw1rr", {"beamSpring":5501000,"beamDamp":15}],
          {"breakGroup":"wheel_FL"},
          ["fh1l","fw1l", {"name":"axle_FL"}],
          ["fh2l","fw1l"],
          ["fh3l","fw1l", {"beamSpring":10501000,"beamDamp":15}],
          ["fh6l","fw1l", {"beamSpring":5501000,"beamDamp":15}],
          ["fh1l","fw1ll"],
          ["fh2l","fw1ll"],
          ["fh3l","fw1ll", {"beamSpring":10501000,"beamDamp":15}],
          ["fh6l","fw1ll", {"beamSpring":5501000,"beamDamp":15}],
          {"breakGroup":""},
          {"optional":false},

          //lower arm
          {"beamSpring":16001000,"beamDamp":1500},
          {"beamDeform":61000,"beamStrength":350000},
          {"breakGroup":"lower_arm_FR"},
          ["fx2r","fh1r", {"beamPrecompression":"$=1+(1-$caster_FR)*0.3","beamPrecompressionTime":0.5,"dampCutoffHz":500}],
          {"breakGroup":"lower_arm_FL"},
          ["fx2l","fh1l", {"beamPrecompression":"$=1+(1-$caster_FR)*0.3","beamPrecompressionTime":0.5,"dampCutoffHz":500}],
          //torque arm
          {"beamSpring":12001000,"beamDamp":1500},
          {"beamDeform":62000,"beamStrength":70000},
          {"breakGroup":"torque_arm_FR"},
          ["fx1r","fh1r", {"beamPrecompression":"$caster_FR","beamPrecompressionTime":0.5,"dampCutoffHz":500}],
          {"breakGroup":"torque_arm_FL"},
          ["fx1l","fh1l", {"beamPrecompression":"$caster_FR","beamPrecompressionTime":0.5,"dampCutoffHz":500}],
          {"breakGroup":""},

          //stays unbroken to keep coilover from stretching after control arm breaks
          {"beamSpring":3001000,"beamDamp":120},
          {"beamDeform":34000,"beamStrength":350000},
          ["fh1r","fh4r"],
          ["fh1l","fh4l"],
          ["fx2r","fh4r"],
          ["fx2l","fh4l"],
          //["fx2r","fh5r"],
          //["fx2l","fh5l"]
          //["fh7l", "fh4l"],
          //["fh7l", "fh1l"],
          //["fh7l", "fx2l"],
          //["fh7r", "fh4r"],
          //["fh7r", "fh1r"],
          //["fh7r", "fx2r"],
          ["arbf3r", "fh1r"],
          ["arbf3l", "fh1l"],
          ["arbf3r", "fx2r"],
          ["arbf3l", "fx2l"],

          {"beamSpring":4501000,"beamDamp":520},
          {"beamDeform":54000,"beamStrength":350000},

          //["fh1r","fh5r", {"dampCutoffHz":500}],
          //["fh1l","fh5l", {"dampCutoffHz":500}],

          //["fh7l", "fh5l", {"dampCutoffHz":500}],
          //["fh7r", "fh5r", {"dampCutoffHz":500}],
          {"beamSpring":5501000,"beamDamp":720},
          //["arbf3r", "fh5r", {"dampCutoffHz":500}],
          //["arbf3l", "fh5l", {"dampCutoffHz":500}],
          {"beamSpring":8501000,"beamDamp":420},
          //["fh4r","fh5r", {"dampCutoffHz":500}],
          //["fh4l","fh5l", {"dampCutoffHz":500}],
          {"beamSpring":2001000,"beamDamp":100},

          ["arbf3r", "fh4r"],
          ["arbf3l", "fh4l"],

          //["arbf3r", "fh7r"],
          //["arbf3l", "fh7l"],

          //upper arm
          {"beamSpring":6001000,"beamDamp":1000},
          {"beamDeform":61000,"beamStrength":40000},
          //camber adjust
          {"breakGroup":"upper_arm_FR"},
          ["fh2r","fx3r", {"beamPrecompression":"$=$camber_FR+(1-$caster_FR)","beamPrecompressionTime":0.5,"dampCutoffHz":500}],
          ["fh2r","fx4r", {"beamPrecompression":"$=$camber_FR-(1-$caster_FR)","beamPrecompressionTime":0.5,"dampCutoffHz":500}],
          {"breakGroup":"upper_arm_FL"},
          ["fh2l","fx3l", {"beamPrecompression":"$=$camber_FR+(1-$caster_FR)","beamPrecompressionTime":0.5,"dampCutoffHz":500}],
          ["fh2l","fx4l", {"beamPrecompression":"$=$camber_FR-(1-$caster_FR)","beamPrecompressionTime":0.5,"dampCutoffHz":500}],
          {"beamPrecompression":1.0},
          {"breakGroup":""},

          //front limiters
          {"deformLimitExpansion":""},
          {"beamPrecompression":0.7, "beamType":"|SUPPORT", "beamLongBound":3},
          {"beamSpring":8001000,"beamDamp":600,"beamDeform":125000,"beamStrength":"FLT_MAX"},
          //firewall
          {"optional":true},
          //{"breakGroupType":1},
          //{"breakGroup":"wheel_FR"},
          ["fw1rr","f19rr"],
          ["fw1rr","f1rr"],
          ["fw1rr","f1r"],
          ["fw1rr","f5r"],
          ["fw1r","f1rr"],
          ["fw1r","f5r"],
          //{"breakGroup":"wheel_FL"},
          ["fw1ll","f19ll"],
          ["fw1ll","f1ll"],
          ["fw1ll","f1l"],
          ["fw1ll","f5l"],
          ["fw1l","f1ll"],
          ["fw1l","f5l"],
          //{"breakGroup":""},
          //{"breakGroupType":0},
          {"optional":false},

          {"beamPrecompression":0.8},
          ["fh1r","f5r"],
          ["fh1l","f5l"],
          ["fh1r","f6r"],
          ["fh1l","f6l"],
          ["fh1r","f6rr"],
          ["fh1l","f6ll"],
          ["fh3r","f5r"],
          ["fh3l","f5l"],
          ["fh3r","f1r"],
          ["fh3l","f1l"],
          ["fh4r","f1r"],
          ["fh4l","f1l"],
          ["fh4r","f1rr"],
          ["fh4l","f1ll"],

          //steering anti invert
          {"beamPrecompression":1, "beamType":"|SUPPORT", "beamLongBound":4},
          {"beamSpring":5001000,"beamDamp":350,"beamDeform":120000,"beamStrength":100000},
          {"beamPrecompression":0.85},
          ["fh6r","fx2r"],
          ["fh6l","fx2l"],
          {"beamPrecompression":0.88},
          ["fh3r","fx1r"],
          ["fh3l","fx1l"],
          {"beamPrecompression":0.78},
          ["fh3r","fx2r"],
          ["fh3l","fx2l"],
          {"beamPrecompression":1},

          //suspension anti-invert
          {"beamSpring":0,"beamDamp":0,"beamDeform":175000,"beamStrength":100000},
          {"beamLimitSpring":5001000,"beamLimitDamp":250},
          {"beamPrecomprssion":1, "beamType":"|BOUNDED", "beamLongBound":0.15, "beamShortBound":0.18},
          ["fh2r","fx1r"],
          ["fh2l","fx1l"],
          ["fh2r","fx2r"],
          ["fh2l","fx2l"],
          {"beamPrecompression":1, "beamType":"|BOUNDED", "beamLongBound":0.13, "beamShortBound":0.2},
          ["fh4r","fx3r"],
          ["fh4l","fx3l"],
          ["fh4r","fx4r"],
          ["fh4l","fx4l"],

          //suspension travel hard limit
          {"beamPrecompression":1, "beamType":"|BOUNDED", "beamLongBound":1, "beamShortBound":1},
          {"beamSpring":1,"beamDamp":100,"beamDeform":15000,"beamStrength":150000},
          {"beamLimitSpring":1001000,"beamLimitDamp":500},
          {"breakGroup":"strut_FR"},
          ["fh4r","fs1r", {"longBoundRange":0.1,"shortBoundRange":0.11,"boundZone":0.01,"beamLimitDampRebound":500,"dampCutoffHz":500}],
          {"breakGroup":"strut_FL"},
          ["fh4l","fs1l", {"longBoundRange":0.1,"shortBoundRange":0.11,"boundZone":0.01,"beamLimitDampRebound":500,"dampCutoffHz":500}],
          {"breakGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"deformLimitExpansion":1.1},
    ],
    "triangles": [
          ["id1:","id2:","id3:"],
          //front subframe
          {"dragCoef":6},


          //front suspension
          {"dragCoef":0},
          {"triangleType":"NONCOLLIDABLE"},
          ["fx1r", "fh4r", "fx2r"],
          ["fh4r", "fh1r", "fx2r"],
          ["fh4r", "fx1r", "fh1r"],
          ["fh3r", "fh1r", "fh6r"],
          ["fh6r", "fh2r", "fh3r"],

          ["fh4l", "fx1l", "fx2l"],
          ["fh1l", "fh4l", "fx2l"],
          ["fx1l", "fh4l", "fh1l"],
          ["fh1l", "fh3l", "fh6l"],
          ["fh2l", "fh6l", "fh3l"],
          {"triangleType":"NORMALTYPE"},
    ],
    "pressureWheels": [
            ["name","hubGroup","group","node1:","node2:","nodeS","nodeArm:","wheelDir"],
            //cancel out brake properties
            {"brakeTorque":0},
            {"parkingTorque":0},
            {"enableBrakeThermals":false},
            {"brakeDiameter":false},
            {"brakeMass":false},
            {"brakeType":false},
            {"rotorMaterial":false},
            {"brakeVentingCoef":false},
    ],
},
"ARaz1_wheeldata_F": {
    "information":{
        "authors":"BeamNG",
        "name":"Front Spindles",
        "value":100,
    },
    "slotType" : "ARaz1_wheeldata_F",
    "pressureWheels": [
        ["name","hubGroup","group","node1:","node2:","nodeS","nodeArm:","wheelDir"],
        //front
        {"selfCollision":false},
        {"collision":true},
        {"hubcapBreakGroup":"hubcap_FR"},
        {"hubcapGroup":"hubcap_FR"},
        {"axleBeams":["axle_FR"]},
        //["FR", "wheel_FR", "tire_FR", "fw1rr", "fw1r", 9999, "fh6r", 1, {"torqueCoupling:":"fh1r","torqueArm:":"fh2r","torqueArm2:":"fh3r","torqueJointNode1:":"tra3","torqueJointNode2:":"tra2","steerAxisUp:":"fh2r","steerAxisDown:":"fh1r"}],
        ["FR", "wheel_FR", "tire_FR", "fw1rr", "fw1r", 9999, "fh6r", 1, {"torqueCoupling:":"fh1r","torqueArm:":"fh2r","torqueArm2:":"fh3r","steerAxisUp:":"fh2r","steerAxisDown:":"fh1r"}],
        {"hubcapBreakGroup":"hubcap_FL"},
        {"hubcapGroup":"hubcap_FL"},
        {"axleBeams":["axle_FL"]},
        //["FL", "wheel_FL", "tire_FL", "fw1ll", "fw1l", 9999, "fh6l", -1, {"torqueCoupling:":"fh1l","torqueArm:":"fh2l","torqueArm2:":"fh3l","torqueJointNode1:":"tra2","torqueJointNode2:":"tra3","steerAxisUp:":"fh2l","steerAxisDown:":"fh1l"}],
        ["FL", "wheel_FL", "tire_FL", "fw1ll", "fw1l", 9999, "fh6l", -1, {"torqueCoupling:":"fh1l","torqueArm:":"fh2l","torqueArm2:":"fh3l","steerAxisUp:":"fh2l","steerAxisDown:":"fh1l"}],
        {"selfCollision":true},
        {"axleBeams":[]},{"disableMeshBreaking":false,"disableTriangleBreaking":false},
        {"hubcapBreakGroup":""},
        {"hubcapGroup":""},
        {"enableHubcaps":false},
        {"enableTireLbeams":false},
        {"enableTireSideReinfBeams":false},
        {"enableTireReinfBeams":false},
        {"enableTreadReinfBeams":false},
        {"enableTirePeripheryReinfBeams":false},
        {"loadSensitivitySlope":""},
        {"noLoadCoef":""},
        {"fullLoadCoef":""},
        {"frictionCoef":""},
        {"slidingFrictionCoef":""},
        {"softnessCoef":0.5},
        {"treadCoef":1.0},
    ],
    "powertrain" : [
        ["type", "name", "inputName", "inputIndex"],
        ["shaft", "spindleFL", "wheelaxleFL", 1, {"connectedWheel":"FL", "breakTriggerBeam":"axle_FL", "uiName":"Front Left Axle", "friction":0.8, "dynamicFriction":0.0015}],
        ["shaft", "spindleFR", "wheelaxleFR", 1, {"connectedWheel":"FR", "breakTriggerBeam":"axle_FR", "uiName":"Front Right Axle", "friction":0.8, "dynamicFriction":0.0015}],
    ],
},
"ARaz1_coilover_F": {
    "information":{
        "authors":"BeamNG",
        "name":"Front Struts",
        "value":250,
    },
    "slotType" : "ARaz1_coilover_F",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["ARaz1_coilover_F", ["ARaz1_shockbottom_F","ARaz1_shocktop_F"]],
    ],
    "beams": [
          ["id1:", "id2:"],
          //front springs with soft initial bump stop
          {"beamPrecompression":1, "beamType":"|BOUNDED", "beamLongBound":1, "beamShortBound":1},
          {"beamDeform":19500,"beamStrength":95000},
          {"beamSpring":34200,"beamDamp":0},
          {"beamLimitSpring":46800,"beamLimitDamp":1000},
          {"breakGroup":"strut_FR"},
          //MR 0.7
          ["fh4r","fs1r", {"name":"spring_FR","precompressionRange":0.085,"longBoundRange":0.085,"shortBoundRange":0.055,"boundZone":0.05,"beamLimitDampRebound":0,"dampCutoffHz":500,
              "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":0.3,"attackFactor":10,"volumeFactor":2.0,"decayFactor":10,"noiseFactor":0.01,"pitchFactor":0.2,"maxStress":1000}],
          {"breakGroup":"strut_FL"},
          ["fh4l","fs1l", {"name":"spring_FL","precompressionRange":0.085,"longBoundRange":0.085,"shortBoundRange":0.055,"boundZone":0.05,"beamLimitDampRebound":0,"dampCutoffHz":500,
              "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":0.3,"attackFactor":10,"volumeFactor":2.0,"decayFactor":10,"noiseFactor":0.01,"pitchFactor":0.2,"maxStress":1000}],
          //shocks
          //MR 0.92
          {"beamSpring":0,"beamDamp":2800},
          {"beamLimitSpring":0,"beamLimitDamp":0},
          {"breakGroup":"strut_FR"},
          ["fh1r","fs1r", {"name":"damper_FR","beamDampFast":1400,"beamDampRebound":4650,"beamDampReboundFast":2700,"beamDampVelocitySplit":0.1,"dampCutoffHz":500}],
          {"breakGroup":"strut_FL"},
          ["fh1l","fs1l", {"name":"damper_FL","beamDampFast":1400,"beamDampRebound":4650,"beamDampReboundFast":2700,"beamDampVelocitySplit":0.1,"dampCutoffHz":500}],
          //high speed choking
          {"beamSpring":0,"beamDamp":0},
          ["fh1r","fs1r", {"beamDampFast":5000,"beamDampRebound":0,"beamDampReboundFast":0,"beamDampVelocitySplit":2,"dampCutoffHz":500}],
          ["fh1l","fs1l", {"beamDampFast":5000,"beamDampRebound":0,"beamDampReboundFast":0,"beamDampVelocitySplit":2,"dampCutoffHz":500}],
          //harder bump stop
          {"beamSpring":0,"beamDamp":0},
          {"beamLimitSpring":201000,"beamLimitDamp":8000},
          {"breakGroup":"strut_FR"},
          ["fh1r","fs1r", {"longBoundRange":0.04,"shortBoundRange":0.04,"boundZone":0.04,"beamLimitDampRebound":0,"dampCutoffHz":500}],
          {"breakGroup":"strut_FL"},
          ["fh1l","fs1l", {"longBoundRange":0.04,"shortBoundRange":0.04,"boundZone":0.04,"beamLimitDampRebound":0,"dampCutoffHz":500}],
          {"breakGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"ARaz1_coilover_F_race": {
    "information":{
        "authors":"BeamNG",
        "name":"Race Front Coilovers",
        "value":950,
    },
    "slotType" : "ARaz1_coilover_F",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["ARaz1_coilover_F", ["ARaz1_shockbottom_F","ARaz1_shocktop_F"]],
    ],
    "variables": [
        ["name", "type", "unit", "category", "default", "min", "max", "title", "description"],
        ["$springheight_F_race", "range", "+m", "Suspension", 0, -0.06, 0.04, "Spring Height", "Raise or lower the suspension height", {"stepDis":0.005, "subCategory":"Front"}],
        ["$spring_F_race", "range", "N/m", "Suspension", 90000, 10000, 150000, "Spring Rate", "Spring stiffness", {"stepDis":500, "subCategory":"Front"}]
        ["$damp_bump_F_race", "range", "N/m/s", "Suspension", 4100, 500, 10000, "Bump Damping", "Damper rate in compression", {"stepDis":100, "subCategory":"Front"}]
        ["$damp_rebound_F_race", "range", "N/m/s", "Suspension", 9600, 500, 20000, "Rebound Damping", "Damper rate in extension", {"stepDis":100, "subCategory":"Front"}]
    ],
    "beams": [
          ["id1:", "id2:"],
          //front springs without soft bump stop
          {"beamType":"|NORMAL"},
          {"beamDeform":19500,"beamStrength":95000},
          {"beamSpring":"$spring_F_race","beamDamp":0},
          //{"beamSpring":0,"beamDamp":0},
          {"breakGroup":"strut_FR"},
          //MR 0.7
          ["fh4r","fs1r", {"name":"spring_FR", "precompressionRange":"$=($springheight_F_race + 0.005) * 0.7",
              "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":0.65,"attackFactor":20,"volumeFactor":2.3,"decayFactor":30,"noiseFactor":0.01,"pitchFactor":1.0,"maxStress":1200}],
          {"breakGroup":"strut_FL"},
          ["fh4l","fs1l", {"name":"spring_FL", "precompressionRange":"$=($springheight_F_race + 0.005) * 0.7",
              "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":0.65,"attackFactor":20,"volumeFactor":2.3,"decayFactor":30,"noiseFactor":0.01,"pitchFactor":1.0,"maxStress":1200}],
          //dampers
          {"beamPrecompression":1, "beamType":"|BOUNDED", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":0,"beamDamp":"$damp_bump_F_race"},
          {"beamLimitSpring":0,"beamLimitDamp":0},
          //MR 0.92
          {"breakGroup":"strut_FR"},
          ["fh1r","fs1r", {"name":"damper_FR","beamDampRebound":"$damp_rebound_F_race","beamDampVelocitySplit":0.05,"beamDampVelocitySplitRebound":0.1,"beamDampFast":"$=$damp_bump_F_race / 2","beamDampReboundFast":"$=$damp_rebound_F_race / 2","dampCutoffHz":500}],
          {"breakGroup":"strut_FL"},
          ["fh1l","fs1l", {"name":"damper_FL","beamDampRebound":"$damp_rebound_F_race","beamDampVelocitySplit":0.05,"beamDampVelocitySplitRebound":0.1,"beamDampFast":"$=$damp_bump_F_race / 2","beamDampReboundFast":"$=$damp_rebound_F_race / 2","dampCutoffHz":500}],
          //bump and rebound stops
          {"beamPrecompression":1, "beamType":"|BOUNDED"},
          {"beamSpring":0,"beamDamp":0},
          {"beamLimitSpring":201000,"beamLimitDamp":8000},
          {"breakGroup":"strut_FR"},
          ["fh1r","fs1r", {"longBoundRange":0.0,"shortBoundRange":0.095,"boundZone":0.03,"beamLimitDampRebound":0,"dampCutoffHz":500}],
          {"breakGroup":"strut_FL"},
          ["fh1l","fs1l", {"longBoundRange":0.0,"shortBoundRange":0.095,"boundZone":0.03,"beamLimitDampRebound":0,"dampCutoffHz":500}],
          {"breakGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"ARaz1_coilover_F_rally": {
    "information":{
        "authors":"BeamNG",
        "name":"Rally Front Coilovers",
        "value":1050,
    },
    "slotType" : "ARaz1_coilover_F",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["ARaz1_coilover_F", ["ARaz1_shockbottom_F","ARaz1_shocktop_F"]],
    ],
    "variables": [
        ["name", "type", "unit", "category", "default", "min", "max", "title", "description"],
        ["$springheight_F_rally", "range", "+m", "Suspension", 0, -0.04, 0.06, "Spring Height", "Raise or lower the suspension height", {"stepDis":0.005, "subCategory":"Front"}],
        ["$spring_F_rally", "range", "N/m", "Suspension", 48000, 10000, 60000, "Spring Rate", "Spring stiffness", {"stepDis":500, "subCategory":"Front"}]
        ["$damp_bump_F_rally", "range", "N/m/s", "Suspension", 3600, 500, 7500, "Bump Damping", "Damper rate in compression", {"stepDis":100, "subCategory":"Front"}]
        ["$damp_bump_F_fast_rally", "range", "N/m/s", "Suspension", 2700, 500, 15000, "Fast Bump Damping", "Damper rate in fast compression", {"stepDis":100, "subCategory":"Front"}]
        ["$damp_rebound_F_rally", "range", "N/m/s", "Suspension", 5800, 500, 7500, "Front Rebound Damping", "Damper rate in extension", {"stepDis":100, "subCategory":"Front"}]
        ["$damp_rebound_F_fast_rally", "range", "N/m/s", "Suspension", 3400, 500, 10000, "Fast Rebound Damping", "Damper rate in fast extension", {"stepDis":100,"subCategory":"Front"}]
    ],
    "beams": [
          ["id1:", "id2:"],
          //front springs
          {"beamType":"|NORMAL"},
          {"beamDeform":20000,"beamStrength":115000},
          {"beamSpring":"$spring_F_rally","beamDamp":0},
          //{"beamSpring":0,"beamDamp":0},
          //MR 0.7
          {"breakGroup":"strut_FR"},
          ["fh4r","fs1r", {"name":"spring_FR", "precompressionRange":"$=($springheight_F_rally + 0.10) * 0.7",
              "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":0.6,"attackFactor":14,"volumeFactor":1.8,"decayFactor":8,"noiseFactor":0.01,"pitchFactor":0.7,"maxStress":1000}],
          {"breakGroup":"strut_FL"},
          ["fh4l","fs1l", {"name":"spring_FL", "precompressionRange":"$=($springheight_F_rally + 0.10) * 0.7",
              "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":0.6,"attackFactor":14,"volumeFactor":1.8,"decayFactor":8,"noiseFactor":0.01,"pitchFactor":0.7,"maxStress":1000}],
          //shocks
          {"beamPrecompression":1, "beamType":"|BOUNDED", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":0, "beamLimitSpring":0,"beamLimitDamp":0},
          //MR 0.92
          {"breakGroup":"strut_FR"},
          ["fh1r","fs1r",
                {
                "name":"damper_FR",
                "beamDamp":"$=$damp_bump_F_rally"
                "beamDampRebound":"$=$damp_rebound_F_rally",
                "beamDampVelocitySplit":0.22,
                "beamDampVelocitySplitRebound":0.1,
                "beamDampFast":"$=$damp_bump_F_fast_rally",
                "beamDampReboundFast":"$=$damp_rebound_F_fast_rally",
                "dampCutoffHz":400
                }
          ],
          {"breakGroup":"strut_FL"},
          ["fh1l","fs1l",
                {
                "name":"damper_FL",
                "beamDamp":"$=$damp_bump_F_rally"
                "beamDampRebound":"$=$damp_rebound_F_rally",
                "beamDampVelocitySplit":0.22,
                "beamDampVelocitySplitRebound":0.1,
                "beamDampFast":"$=$damp_bump_F_fast_rally",
                "beamDampReboundFast":"$=$damp_rebound_F_fast_rally",
                "dampCutoffHz":400
                }
          ],
          //hydraulic bump stop
          {"beamPrecompression":1, "beamType":"|BOUNDED"},
          {"beamSpring":0,"beamDamp":0},
          {"beamLimitSpring":10000,"beamLimitDamp":14000},
          {"breakGroup":"strut_FR"},
          ["fh1r","fs1r", {"longBoundRange":1,"shortBoundRange":0.055,"boundZone":0.02,"beamLimitDampRebound":1000,"dampCutoffHz":250}],
          {"breakGroup":"strut_FL"},
          ["fh1l","fs1l", {"longBoundRange":1,"shortBoundRange":0.055,"boundZone":0.02,"beamLimitDampRebound":1000,"dampCutoffHz":250}],
          {"breakGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"ARaz1_swaybar_F": {
    "information":{
        "authors":"BeamNG",
        "name":"Front Sway Bar",
        "value":100,
    },
    "slotType" : "ARaz1_swaybar_F",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["ARaz1_swaybar_F", ["ARaz1_swaybar_F"],[]],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //anti-roll
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":"ARaz1_swaybar_F"},
         {"selfCollision":false},
         {"collision":true},
         {"nodeWeight":1.9},
         //front anti-roll
         ["arbf1r", -0.22986, -1.02355, 0.21052],
         ["arbf1l", 0.22986, -1.02355, 0.21052],
         ["arbf2r", -0.40226, -1.21894, 0.24356],
         ["arbf2l", 0.40226, -1.21894, 0.24356],
         {"group":""},
    ],
    "torsionbars": [
        ["id1:", "id2:", "id3:", "id4:"],
        //15mm 435.6
        //16mm 563.9
        //17mm 718.6
        //18mm 903.2
        //19mm 1121.2
        //20mm 1376.5
        //21mm 1673.2
        //22mm 2015.4
        //23mm 2407.6
        //24mm 2854.5
        //25mm 3360.8
        {"spring":903.2, "damp":5, "deform":10000, "strength":9999999},
        ["arbf2r", "arbf1r", "arbf1l", "arbf2l"],
    ],
    "beams": [
          ["id1:", "id2:"],
          //--ANTI-ROLL--
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
          {"beamSpring":4001000,"beamDamp":100},
          {"beamDeform":15000,"beamStrength":310000},
          //end links
          ["arbf2r","arbf3r"],
          ["arbf2l","arbf3l"],
          //rigifier
          {"beamSpring":3001000,"beamDamp":100},
          {"beamDeform":15000,"beamStrength":310000},
          ["arbf1r","arbf1l"],
          ["arbf1r","arbf2r"],
          ["arbf1l","arbf2l"],
          ["arbf1r","arbf2l"],
          ["arbf1l","arbf2r"],
          //attach to subframe

          ["arbf1r", "fx2r"],
          ["arbf1r", "fx6r"],
          ["arbf1r", "fx6l"],
          ["arbf1r", "fx2l"],

          ["arbf1l", "fx2l"],
          ["arbf1l", "fx6l"],
          ["arbf1l", "fx6r"],
          ["arbf1l", "fx2r"],

          {"breakGroup":"subframemount_FRR"},
          ["f1r", "arbf1r"],
          ["arbf1r", "fx4r"],
          ["arbf1r", "f5r"],
          //["arbf1r", "f1l"],
          //
          {"breakGroup":"subframemount_FRL"},
          ["f1l", "arbf1l"],
          ["arbf1l", "fx4l"],
          ["arbf1l", "f5l"],
          //["arbf1l", "f1r"],
          {"breakGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"ARaz1_steering": {
    "information":{
        "authors":"BeamNG",
        "name":"Steering",
        "value":110,
    },
    "slotType" : "ARaz1_steering",
    "slots": [
        ["type", "default", "description"],
        ["ARaz1_power_steering","", "Power Steering"],
    ],
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["ARaz1_tierod", ["ARaz1_tierod_F","ARaz1_steeringbox_F","ARaz1_hub_FR","ARaz1_hub_FL"]],
    ],
    "rails": {
        "steeringrack":{"links:":["fh8r", "fh8l"], "broken:":[], "looped":false, "capped":true},
    },
    "slidenodes": [
        ["id:", "railName", "attached", "fixToRail", "tolerance", "spring", "strength", "capStrength"],
        ["fx5r", "steeringrack", true, true, 0.0, 12001000, "FLT_MAX", "FLT_MAX"],
        ["fx5l", "steeringrack", true, true, 0.0, 12001000, "FLT_MAX", "FLT_MAX"],
    ],
    "variables": [
        ["name", "type", "unit", "category", "default", "min", "max", "title", "description"],
        ["$toe_FR", "range", "", "Wheel Alignment", 1.001, 0.98, 1.02, "Toe Adjust", "Adjusts the wheel toe-in angle", {"subCategory":"Front"}],
        ["$steer_center_F", "range", "", "Wheel Alignment", 0, -0.002, 0.002, "Toe Left/Right Trim", "Fine tunes the centerpoint of the steering", {"subCategory":"Front"}]
    ],
    "nodes": [
        ["id", "posX", "posY", "posZ"],
        //--steering rod--
        {"selfCollision":false},
        {"collision":true},
        {"nodeMaterial":"|NM_METAL"},
        {"frictionCoef":0.5},
        {"group":"ARaz1_tierod_F"},
        {"nodeWeight":5.5},
        ["fh8r", -0.29721, -1.10471, 0.26082],
        ["fh8l", 0.29721, -1.10471, 0.26082],
        {"group":""},
    ],
    "beams": [
          ["id1:","id2:"],
          {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
          {"beamSpring":8001000,"beamDamp":100,"beamDeform":81000,"beamStrength":174000},
          ["fh8r","fh8l"],
          //toe (below 1 = toe out, above 1 = toe in)
          {"beamSpring":12001000,"beamDamp":100},
          {"beamDeform":71000,"beamStrength":154000},
          ["fh3r","fh8r", {"beamPrecompression":"$=$toe_FR-$steer_center_F","beamPrecompressionTime":0.5}],
          ["fh3l","fh8l", {"beamPrecompression":"$=$toe_FR+$steer_center_F","beamPrecompressionTime":0.5}],
          //steering damper
          {"beamPrecompression":1.0, "beamType":"|BOUNDED", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamLimitSpring":0,"beamLimitDamp":0},
          {"beamSpring":0},
          {"beamDamp":70},
          ["fh3r","fx6r", {"beamDampVelocitySplit":0.1,"beamDampFast":750,"dampCutoffHz":750}],
          ["fh3l","fx6l", {"beamDampVelocitySplit":0.1,"beamDampFast":750,"dampCutoffHz":750}],
          ["fh8r","fx2r", {"beamDampVelocitySplit":0.1,"beamDampFast":750,"dampCutoffHz":750}],
          ["fh8l","fx2l", {"beamDampVelocitySplit":0.1,"beamDampFast":750,"dampCutoffHz":750}],
          {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
    ],
    "triangles": [
          ["id1:","id2:","id3:"],
          {"triangleType":"NONCOLLIDABLE"},
          {"dragCoef":0},
          ["fx2r", "fh8r", "fx2l"],
          ["fx2r", "fh8l", "fx2l"],
          {"triangleType":"NORMALTYPE"},
    ],
    "hydros": [
        ["id1:","id2:"],
        {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
        {"beamSpring":7001000,"beamDamp":40,"beamDeform":"FLT_MAX","beamStrength":124000},
        ["fh8r","fx5l", {"factor":-0.108,"steeringWheelLock":540,"inRate":0.7,"outRate":0.7}],
        ["fh8l","fx5r", {"factor":0.108,"steeringWheelLock":540,"inRate":0.7,"outRate":0.7}],
        {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
    ],
    "input": {
        "FFBcoef":"$=$ffbstrength*9.5",
    },
},
}