{
"tire_R_235_55_19_standard": {
    "information":{
        "authors":"BeamNG",
        "name":"235/55R19 Standard Rear Tires",
        "value":270,
    },
    "slotType" : "tire_R_19x8",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["tire_01a_18x8_27_5", ["wheel_RR","tire_RR"], [], {"pos":{"x":-0.48, "y":0.0, "z":0.0}, "rot":{"x":0, "y":0, "z":180}, "scale":{"x":0.98, "y":1.05, "z":1.05}}],
        ["tire_01a_18x8_27_5", ["wheel_RL","tire_RL"], [], {"pos":{"x": 0.48, "y":0.0, "z":0.0}, "rot":{"x":0, "y":0, "z":0},   "scale":{"x":0.98, "y":1.05, "z":1.05}}],
    ],
    "variables": [
        ["name", "type", "unit", "category", "default", "min", "max", "title", "description"],
        ["$tirepressure_R", "range", "psi", "Wheels", 30, 0, 50, "Tire Pressure", "Relative to atmospheric pressure", {"subCategory":"Rear"}],
    ],
    "pressureWheels": [
        ["name","hubGroup","group","node1:","node2:","nodeS","nodeArm:","wheelDir"],
        {"disableMeshBreaking":false,"disableHubMeshBreaking":false},
        {"hasTire":true},
        {"enableTireReinfBeams":false},
        {"enableTireLbeams":true},
        {"enableTireSideReinfBeams":false},
        {"enableTreadReinfBeams":true},
        {"enableTirePeripheryReinfBeams":true},

        //general settings
        {"radius":0.367},
        {"tireWidth":0.215},

        //tire options
        {"wheelSideBeamSpring":"$=$tirepressure_R*1050","wheelSideBeamDamp":25},
        {"wheelSideBeamSpringExpansion":421000,"wheelSideBeamDampExpansion":35},
        {"wheelSideTransitionZone":0.1,"wheelSideBeamPrecompression":0.985},

        {"wheelReinfBeamSpring":31000,"wheelReinfBeamDamp":190},
        {"wheelReinfBeamDampCutoffHz":500,"wheelReinfBeamPrecompression":0.98},

        {"wheelTreadBeamSpring":51000,"wheelTreadBeamDamp":80},
        {"wheelTreadBeamDampCutoffHz":500,"wheelTreadBeamPrecompression":0.98},

        {"wheelTreadReinfBeamSpring":151000,"wheelTreadReinfBeamDamp":60},
        {"wheelTreadReinfBeamDampCutoffHz":500,"wheelTreadReinfBeamPrecompression":0.98},

        {"wheelPeripheryBeamSpring":41000,"wheelPeripheryBeamDamp":35},
        {"wheelPeripheryBeamDampCutoffHz":500,"wheelPeripheryBeamPrecompression":0.98},

        {"wheelPeripheryReinfBeamSpring":121000,"wheelPeripheryReinfBeamDamp":35},
        {"wheelPeripheryReinfBeamDampCutoffHz":500,"wheelPeripheryReinfBeamPrecompression":0.98},

        //general tire values
        {"nodeWeight":0.155},
        {"nodeMaterial":"|NM_RUBBER"},
        {"triangleCollision":false},
        {"pressurePSI":"$tirepressure_R"},
        {"dragCoef":5},

        //groundmodel friction multipliers
        {"frictionCoef":1.0},
        {"slidingFrictionCoef":1.0},
        //{"stribeckExponent":1.5},
        {"stribeckVelMult":1.2},
        {"treadCoef":0.5},

        //advanced friction values
        {"noLoadCoef":1.39},
        {"loadSensitivitySlope":0.00015},
        {"fullLoadCoef":0.45},
        {"softnessCoef":0.7},

        //deform values
        {"wheelSideBeamDeform":17000,"wheelSideBeamStrength":22000},
        {"wheelTreadBeamDeform":12000,"wheelTreadBeamStrength":16000},
        {"wheelPeripheryBeamDeform":55000,"wheelPeripheryBeamStrength":55000},
    ],
},
}